
                   ::::::::::::::::::::::::::::::::::::::::
                   ::INSTALLING A SUPERNOVA BOOT DISKETTE::
                   ::::::::::::::::::::::::::::::::::::::::


1) Either  make a  backup copy  of your  DOS diskette  (must be version 2.0  or
   higher) or use any diskette that has a copy of command.com on it.

2) Turn on  your computer with the  DOS diskette in drive A:  (Note:  Remember,
   your disk will now become the "boot" disk.)

3) After  the  A>  prompt  appears  remove  your DOS  diskette  and insert  the
   SUPERNOVA diskette into drive A:

4) Type INSTALL and press the <enter> key (or <return>, etc.)

5) The INSTALL program  will explain  itself.  At the  bottom,  in  highlighted
   letters it will ask you to remove the SUPERNOVA disk and insert your  "boot"
   diskette.  Do this, then press any key to continue.

6) A few  seconds  later  your  "boot"  diskette  will be  properly  installed.

